Stormwater Management System: TCNJ Townhouses South

Team Members: Kelly Hommen, Elizabeth Lafferty (PM), Michael Murphy, Charles Stewart Advisors: Dr. Michael Horst and Dr. Vedrana Krstic

TCNJ Senior Project I December 2012

Stormwater Management System: TCNJ Townhouses South



An Analysis Project for Senior Project I

Submitted to the Faculty of the Civil Engineering Department

of The College of New Jersey

Written and Researched by:

Kelly Hommen

Elizabeth Lafferty

Michael Murphy

Charles Stewart

In partial fulfillment of the Bachelor of Science degree in Civil Engineering

December 2012

**Abstract:**

The College of New Jersey’s Townhouses South residences experience water infiltration and persistent dampness in their crawlspaces. Townhouses South is comprised of 26 individual units each of which has a crawlspace extending approximately 3 feet below the surface. Of the 26 units, standing water was detected in the crawlspaces of 15 of them, and all but 6 have noticeable moisture. This study is intended to determine the foremost cause of the water infiltration and propose a solution to maintain the structural integrity of the Townhouses. Through the use of geotechnical, hydrologic, and hydraulic analysis, data was collected to allow for proper analysis and the proposal of adequate solutions. Geotechnical testing was conducted in accordance with ASTM standards, and soil was classified using Burmister classification system to produce a soil profile. The profile is comprised of four stratums; the top three consist of brown sand with trace amounts of silt. The final stratum, located seven feet below the surface, is brown sand with clayley silt. The hydraulic conductivity of the first five feet of the soil profile was determined to be 0.001323 ft/min. A ground water well was installed in close proximity to the most critical crawlspaces and extended to a depth of seven feet below the surface. Although no groundwater table was found, continuous monitoring will occur. With the use of topographic maps, watershed properties were obtained and used in combination with rainfall estimates to predict the volume of infiltrated water for a 2 year, 24 hour storm event. The watershed was divided into two separate areas, impervious and pervious. The areas were found to be 0.98 acres and 0.94 acres, respectively. The computer modeling software HEC-HMS was utilized and returned total absorbed water of 0.12 inches and 2.47 inches for the respective areas. During Senior Project II, designs to remediate this problem will be considered for future use. Potential solutions include an underground storm water collection and recycling system, regrading of the soil surrounding the townhouses, a rooftop rainwater catchment system, and a design for sump pumps in the crawlspaces.

Table of Contents

Fulfillment Pagei

Abstractii

Table of Contentsiii

Table of Figuresiv

Table of Tablesv

Chapter 1: Introduction1

Chapter 2: Team Management *(Elizabeth Lafferty)* 2

Chapter 3: Background *(Elizabeth Lafferty)*

3.1 Overview3

3.2 Best Management Practice Research3

3.3 Site Description3

3.4 Conclusion4

Chapter 4: Soil Analysis *(Kelly Hommen)*

4.1 Overview5

4.2 Soil Sampling6

4.3 Field Testing7

4.4 Groundwater Table Monitoring Well7

4.5 Laboratory Testing9

4.6 Soil Classification13

4.7 Hydraulic Conductivity of Soil13

4.8 Conclusion13

Chapter 5: Hydraulic and Hydrologic Analysis *(Michael Murphy and Charles Stewart)*

5.1 Overview15

5.2 Watershed Delineation15

5.3 Modeling Site Conditions17

5.4 Calculating Lag Time18

5.4.1 SCS Regression Method

5.5 Conclusion19

Chapter 6: Computer Modeling *(Michael Murphy and Charles Stewart)……………………………………*20

Chapter 7: Future Designs (*Elizabeth Lafferty*)23

Chapter 8: Conclusion (*Elizabeth Lafferty*)24

References25

Appendix A: Project Overview26

Team Members

Engineering Standards and Realistic Constraints Form SPI

Realistic Constraints and Engineering Standards Presentation

Safety Essay

Appendix B: Team Management32

Gantt Chart

Weekly Meeting Minutes Example

Contact List

Appendix C: Site Description36

Aerial Photo

Appendix D: Soil Analysis38

Natural Moisture Content Results

Sieve Analysis Results

Laboratory/Field Testing Equations

Typical Values for Hydraulic Conductivity

NJBMP Procedures

Burmister Classification

Lab Data Sheet Example

Appendix E: Hydrologic Analysis 48

Table of Runoff Curve Numbers

NOAA Website Table of Total Rainfall

**Stormwater Management System: TCNJ Townhouses South**

**List of Figures**

Figure 2.1.1: Townhouse South Stormwater Management Website…………………………………………………….2

Figure 3.3.1: Site Location………………………………………………………………………………………………………………….3

Figure 3.3.2: Watersheds………………………………………………………………………………………………………………….4

Figure 4.1.1: Location of Soil Borings, Percolation Tests, and Groundwater Table Monitoring Well….. 5

Figure 4.3.1: Percolation Test……………………………………………………………………………………………………………..7

Figure 4.4.1: Groundwater Monitoring Well (Profile View)……………………………………………………………….8

Figure 4.4.2: Groundwater Monitoring Well………………………………………………………………………………………8

Figure 4.5.1: Grain Size Distribution Curves……………………………………………………………………………………..11

Figure 4.6.1: Soil Profile………………………………………………………………………………………………………………………

Figure 5.2.1: Watershed ………………………………………………………………………………………………………………………16

Figure 5.2.2: Longest Hydraulic Length………………………………………………………………………………………………17

Figure 5.3.1: Soil Type………………………………………………………………………………………………………………………18

Figure 5.3.2: Soil Breakdown…………………………………………………………………………………………………………………18

Figure 6.1: HEC-HMS………………………………………………………………………………………………………………………21

Figure 6.2: HEC-HMS………………………………………………………………………………………………………………………21

Figure 6.3: HEC-HMS………………………………………………………………………………………………………………………22

**Stormwater Management System: TCNJ Townhouses South**

**List of Tables**

Table 4.5.1: Natural Moisture Content Results…………………………………………………………………………….9

Table 4.5.2: Results for Atterberg Limits………………………………………………………………………………………

Table 4.7.1: Relationship of Field Calculations to Empirical Values………………………………………………13

Table 6.1: Land Use and Design Storm Return Period …………………………………………………………………20